For 1990-2009 cars

### Removal Procedure

1. Apply the parking brake.
2. Move the shift control lever rearward to one of the low gear positions.
3. Remove the 2 bolts.
4. Remove the knob from the shift control lever.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the knob and bolts to the shift control lever and tighten to 2 N·m (18 lb in).
2. Place the shift control lever in the PARK position.