For 1990-2009 cars

### Removal Procedure

1. Turn the ignition switch to the off position.
2. Disconnect the electronic throttle control (ETC) connector from the accelerator pedal.
3. Remove the 3 accelerator pedal retaining bolts.
4. Remove the accelerator pedal.

### Installation Procedure

1. Position the accelerator pedal.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the 3 accelerator pedal retaining nuts.

Tighten

• | Tighten the upper accelerator pedal retaining bolts (1) to 10 N·m (89 lb in).

• | Tighten the lower accelerator pedal retaining bolt (2) to 23 N·m (17 lb ft).

3. Connect the ETC connector to the accelerator pedal.