For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the C-pillar trim panel.
3. Remove the seat belt anchor bolt.
4. Remove the rear window shelf panel. Refer to Rear Window Shelf Trim Panel Replacement .
5. Remove the seat belt guide from the rear shelf.
6. Remove the bolt and the seat belt retractor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear seat belt retractor and bolt.

Tighten
Tighten the rear seat belt retractor bolts to 38 N·m (28 lb ft).

2. Install the seat belt guide to rear shelf.
3. Install the rear window shelf panel. Refer to Rear Window Shelf Trim Panel Replacement .
4. Install the lower seat belt anchor bolts.

Tighten
Tighten the lower seat belt anchor bolt to 38 N·m (28 lb ft).

5. Install the C-pillar trim panel.
6. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .