For 1990-2009 cars

### Removal Procedure

1. Raise the hood.
2. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .
3. Remove the weatherstrip.
4. Remove the air inlet grille retaining screws, clips, and the 2-piece grille.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the 2-piece grille with the air inlet grille retaining clips and screws.

Tighten
Tighten the air inlet grille screws to 3 N·m (27 lb in).

2. Install the weatherstrip.
3. Install the wiper arms. Refer to Windshield Wiper Arm Replacement .
4. Lower the hood.