For 1990-2009 cars

Table 1: | 3-5 Reverse Clutch Plates Installation
Table 2: | Reluctor Wheel and Piston Installation
Table 3: | 4-5-6 Clutch Piston Installation
Table 4: | 4-5-6 Clutch Fluid Dam Installation
Table 5: | 4-5-6 Clutch Plates Installation
Table 6: | Turbine Shaft Installation

### 3-5 Reverse Clutch Plates Installation

Callout | Component Name
--- | ---
1 | 3-5 Reverse Clutch Apply Plate (Waved)
2 | 3-5 Reverse Clutch Plate (Qty: 3)
3 | 3-5 Reverse Clutch Plate Assembly (Qty: 3)
4 | 3-5 Reverse Clutch Backing Plate
5 | 3-5 Reverse Clutch Backing Plate Ring Retainer Ring

### Reluctor Wheel and Piston Installation

Callout | Component Name
--- | ---
1 | 3-5 Reverse Clutch Piston Dam Seal (Black)
2 | 3-5 Reverse Clutch Piston Inner Seal
3 | 3-5 Reverse Clutch Piston Inner (Reluctor) Seal (Orange)
4 | 3-5 Reverse Clutch Piston Return Spring Assembly
5 | 3-5 Reverse Clutch Piston
6 | Input Shaft Speed Sensor Reluctor Wheel
7 | Input Shaft Speed Sensor Reluctor Ring Retainer Ring Caution: Compress the reluctor wheel just enough to clear the retainer. Over compressing the reluctor wheel will break the alignment tab and the clutch housing. Tip Place the housing assembly onto the input shaft support inside the case. Apply shop air to the clutch fluid feed hole in the case to verify proper piston operation.

#### Special Tool

DT-47694 Piston Spring Compressor

### 4-5-6 Clutch Piston Installation

Callout | Component Name
--- | ---
1 | 4-5-6 Clutch Piston Inner Seal
2 | 4-5-6 Clutch Piston Outer Seal (Large) (Rounded)
3 | 4-5-6 Clutch Piston Outer Seal (DK Blue) (Stepped)
4 | 4-5-6 Clutch Piston Tip

• | DT-47805 prevents the dam seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of DT-47805 to ease the installation of the piston.

• | DT-47951-2 can be used as a pusher if necessary.

#### Special Tool

• | DT-47805 Seal Protector

• | DT-47951-2 Spring Compressor

### 4-5-6 Clutch Fluid Dam Installation

Callout | Component Name
--- | ---
1 | 4-5-6 Clutch Piston Return Spring Assembly
2 | 4-5-6 Clutch Piston Fluid Dam Assembly Tip DT-47951-1 prevents the dam seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of DT-47951-1 to ease the installation of the dam.

#### Special Tool

DT-47951-1 Seal Protector

3 | 4-5-6 Clutch Dam Retaining Ring Tip

• | Leave DT-47951-1 in place while installing the retaining ring.

• | Place the housing assembly onto the input shaft support inside the case. Apply shop air to the clutch fluid feed hole in the case to verify proper piston operation.

#### Special Tool

DT-47951-2 Spring Compressor

### 4-5-6 Clutch Plates Installation

Callout | Component Name
--- | ---
1 | Reaction Carrier Hub Thrust Bearing Assembly
2 | Reaction Carrier Hub Assembly
3 | 4-5-6 Clutch Wave Plate
4 | 4-5-6 Clutch Apply Plate
5 | 4-5-6 Clutch Plate Assembly (Qty: 4)
6 | 4-5-6 Clutch Plate (Qty: 3)
7 | 4-5-6 Clutch Backing Plate
8 | 4-5-6 Clutch Backing Plate Retaining Ring

### Turbine Shaft Installation

Callout | Component Name
--- | ---
1 | Turbine Shaft
2 | Turbine Shaft Retainer Ring Tip Do not re-use the turbine shaft retainer ring.

#### Special Tool

J-5586-A Snap Ring Pliers or equivalent