For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the theft deterrent alarm electrical connector.
3. Remove the theft deterrent alarm bracket mounting bolt.
4. Remove the theft deterrent alarm.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the theft deterrent alarm bracket with the mounting bolt. Make sure that the theft deterrent alarm bracket mounting bolt also fastens the auxiliary fan relay.

Tighten
Tighten the theft deterrent alarm bracket mounting bolt to 11 N·m (97 lb in).

2. Connect the theft deterrent alarm electrical connector.
3. Connect the negative battery cable.