For 1990-2009 cars

### Removal Procedure

1. Remove the door seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement .
2. Remove the inside door handle. Refer to Door Inside Handle Replacement .
3. Disconnect the inside lock rods from the lock.

### Installation Procedure

1. Connect the inside lock rods to the lock.
2. Install the inside door handle. Refer to Door Bottom Auxiliary Sealing Strip Replacement .
3. Install the door seal trim. Refer to Door Inside Handle Replacement .