For 1990-2009 cars

#### Tools Required

J 45004 Fuel Tank Drain Hose

Important: Purge any residual fuel in J 45004 into an approved container prior to use.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the fuel fill cap.
3. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
4. Loosen the fuel fill pipe clamp.
5. Remove the fuel fill pipe from the fuel tank.
6. Insert the J 45004 hose into the tank.
7. Attach the J 45004 hose to the hose used with the hand or air operated pump devise.
8. Using a hand or air operated pump drain as much fuel from the tank as possible.