For 1990-2009 cars

### Removal Procedure

1. Remove the front door escutcheon.
2. Disconnect the mirror electrical connector if the mirror is electronically controlled.
3. Remove the bolts and the outside rearview mirror assembly from the door.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the outside rearview mirror assembly to the door with the screws and tighten to 4.5 N·m (40 lb in).
2. Connect the mirror electrical connector if the mirror is electronically controlled.
3. Install the front door escutcheon.