For 1990-2009 cars

#### Tools Required

J 21104-B (KM-475-B) Weatherstrip Remover Universal or equivalent

### Removal Procedure

1. Lower the front window.
2. Remove the rear deck lid remote switch and the power window/mirror control switch.
3. Disconnect the electrical connectors.
4. Remove the door trim panel screws.
5. Pry off the trim panel using the J 21104-B .
6. Remove the door step lamp.

### Installation Procedure

1. Install the door step lamp.
2. Install the trim panel.
3. Connect the electrical connectors.
4. Install the rear deck lid remote switch and the power window/mirror control switch.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the door trim panel screws.

Tighten
Tighten the door trim panel screws to 2.5 N·m (22 lb in).

6. Raise the front window.