For 1990-2009 cars

## Generator Usage Gasoline Engines

Application | Description
--- | ---
2.0L
Amperage | 85 A
Type | CS-128D
2.5L
Amperage | 120 A
Type | CS-121 DIF

## Generator Usage Diesel Engine

Description | Specification
--- | ---
Unit | Standard
Type | -- | AD237
Capacity | AH | 125
Regulator Type | -- | Multi/Non RVC
Regulator Voltage | V | 14.6 ± 0.25 at Tb=25°C 6,000 RPM 50% Load
Brush

- Length

mm (in)

21.8

- Number

EA

2

- Minimum Length

mm (in)

11.0