For 1990-2009 cars

#### Tools Required

J 21104-B (KM-475-B) Weatherstrip Remover Universal, or equivalent

### Removal Procedure

1. Open the hood.
2. Remove the washer hose from the hood.
3. Remove the retaining clips using the J 21104-B (1).
4. Remove the hood insulation.

### Installation Procedure

1. Install the hood insulation with the retaining clips.
2. Install the washer hose to the hood.
3. Close the hood.