For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the front bumper energy absorber. Refer to Front Bumper Fascia Energy Absorber Replacement.
3. Disconnect the electrical connector.
4. Remove the bolts and the front bumper impact bar.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the front impact bar with the bolts and tighten to 39 N·m (29 lb ft).
2. Connect the electrical connector.
3. Install the front bumper energy absorber. Refer to Front Bumper Fascia Energy Absorber Replacement.
4. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement.