For 1990-2009 cars

### Removal Procedure

1. Remove the rotor. Refer to Front Brake Rotor Replacement .
2. Remove the bolts and the lockwashers for the splash shield from the steering knuckle.
3. Remove the splash shield.

### Installation Procedure

1. Install the splash shield.

Notice: Refer to Fastener Notice in the Preface section.

2. Secure the splash shield to the steering knuckle with the bolts and the lockwashers.

Tighten
Tighten the splash shield-to-steering knuckle bolts to 25 N·m (18 lb ft).

3. Install the rotor. Refer to Front Brake Rotor Replacement .