For 1990-2009 cars

### Removal Procedure

1. Remove the coin storage and the screws.
2. Separate the hood release cable from the hood latch release handle.
3. Carefully pull the instrument panel under cover until the mounting clips are released and the instrument panel under cover.
4. Remove the bolts from the driver side knee bolster.
5. Remove the knee bolster.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the knee bolster with the bolts and tighten to 10 N·m (89 lb in).
2. Install the instrument panel under cover.
3. Connect the hood release cable to the hood latch release handle.
4. Install the coin storage and the screws.