For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 20 N·m | 15 lb ft
Clutch Housing to Transaxle Housing Bolts | 20-25 N·m | 15-18 lb ft
Clutch Release Cylinder Bracket Bolts | 15 N·m | 11 lb ft
Clutch Release Fork Bolt | 20-25 N·m | 15-18 lb ft
Fluid Drain Plug | 6 N·m + 45-180° | 53 lb in + 45-180°
Fluid Level Check Plug | 6 N·m + 45-180° | 53 lb in + 45-180°
Front Damper Bush Bracket Bolts | 65 N·m | 48 lb ft
Input Shaft Retainer Plug | 90-100 N·m | 66-74 lb ft
Interm Shaft Retainer Plug | 90-100 N·m | 66-74 lb ft
Left Upper Transaxle Mounting Bracket Bolts | 40 N·m | 30 lb ft
Lower Transaxle Retaining Bolts | 27-35 N·m | 20-26 lb ft
Output Shaft Retainer Plug | 90-100 N·m | 66-74 lb ft
Rear Transaxle Mounting Bracket Bolts | 65 N·m | 48 lb ft
Shift Control Cable Bracket Bolts | 10-14 N·m | 89-124 lb in
Shift Control Lever Housing Bolt | 8 N·m | 71 lb in
Shift Guide Bolt | 20-25 N·m | 15-18 lb ft
Shift Retaining Bolts | 20-25 N·m | 15-18 lb ft
Speedometer Driven Gear Bolt | 3-5 N·m | 27-44 lb in
Thread Pin | 6-9 N·m | 53-80 lb in
Thrust Bearing Guide Bolts | 8-12 N·m | 71-106 lb in
Transaxle Housing Rear Cover Bolts | 20-25 N·m | 15-18 lb ft
Transaxle Housing to Clutch Housing Bolts | 20-25 N·m | 15-18 lb ft
Upper Transaxle Retaining Bolts | 60-85 N·m | 44-63 lb ft