For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Slide the side turn signal lamp to the left.
3. Remove the side turn signal lamp from the fender.
4. Disconnect the electrical connector.
5. Twist and remove the bulb from the side turn signal lamp.

### Installation Procedure

1. Insert and twist to install the replacement bulb into the side turn signal lamp.
2. Connect the electrical connector.
3. Install the side turn signal lamp into the fender.
4. Connect the negative battery cable.