For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Filter Housing Bolt | 10 N·m | 89 lb in
Alternator Lower Bolt | 35 N·m | 26 lb ft
Alternator Upper Bolt | 35 N·m | 26 lb ft
Battery Rod Clamp Nut | 4 N·m | 35 lb in
Bed Plate Baffle Bolt | 8 N·m | 71 lb in
Bed Plate Inner Bolt | 33 N·m + 135° | 24 lb ft + 135°
Bed Plate Outer Bolt | 23 N·m | 17 lb ft
Cam Sprocket Bolt | 20 N·m | 15 lb in
Camshaft Cap Bolt | 12 N·m | 106 lb in
Camshaft Position (CMP) Sensor | 12 N·m | 106 lb in
Catalytic Converter Heat Shield Nut | 2.5 N·m | 22 lb in
Center Front Suspension Member Bolt | 90 N·m | 66 lb ft
Compressor Retaining Bolt/Nut | 25 N·m | 18 lb ft
Connecting Piece | 20 N·m | 15 lb ft
Connecting Rod Cap Bolt | 20 N·m + 45° + 90° | 15 lb ft + 45° + 90°
Coolant Outlet Port Retaining Bolt | 10 N·m | 89 lb in
Coolant Reservoir Bolt | 4 N·m | 35 lb in
Cooling Fan Assembly Bolt | 4 N·m | 35 lb in
Crankshaft Position (CKP) Sensor Bolt | 6 N·m | 53 lb in
Crankshaft Pulley Bolt | 550 N·m | 406 lb ft
Cylinder Head Bolt | 20 N·m, 25 N·m + 70° + 70° | 15 lb ft, 18 lb ft + 70° + 70°
Cylinder Head Cover Bolt | 13 N·m | 115 lb in
Drive Belt Automatic Tensioner | 25 N·m | 18 lb ft
EGR Adapter Retaining Bolt | 20 N·m | 15 lb ft
EGR Bolt | 25 N·m | 18 lb ft
Engine Beautification Cover Bolt | 10 N·m | 89 lb in
Engine Block Ground Bolt | 20 N·m | 15 lb ft
Engine Block-to-Transaxle Bolt | 72 N·m | 53 lb ft
Engine Coolant Temperature (ECT) Sensor | 17 N·m | 13 lb ft
Engine Mount Bracket Bolt | 51 N·m | 38 lb ft
Engine Mount Bracket Nut | 51 N·m | 38 lb ft
Engine Mount Bracket Support Bolt | 28 N·m | 21 lb ft
Engine Mount Bracket-to-Hydro Mount Nut | 63 N·m | 46 lb ft
Engine Oil Dipstick Tube Bolt | 9 N·m | 80 lb ft
Engine Oil Dipstick Tube Bracket Bolt | 20 N·m | 15 lb ft
Engine Under Cover Retaining Bolt | 23 N·m | 17 lb ft
Evaporative Emission Canister Vapor Pipe Retaining Bolts | 10 N·m | 89 lb in
Exhaust Manifold Heat Shield Bolt | 20 N·m | 15 lb ft
Exhaust Manifold Retaining Nut | 28 N·m | 21 lb ft
Fixed Timing Chain Guide Bolt | 20 N·m | 15 lb ft
Flexible Plate Bolt | 75 N·m | 55 lb ft
Front Damper Bush Bracket Bolt | 65 N·m | 48 lb ft
Front Engine Mount Bracket-to-Damper Bush Bolt | 80 N·m | 59 lb ft
Front Exhaust Pipe Lower Bracket Bolt | 40 N·m | 30 lb ft
Front Exhaust Pipe Nut | 40 N·m | 30 lb ft
Front Exhaust Pipe-to-Front Muffler Nut | 30 N·m | 22 lb ft
Front Muffler Heat Shield Nut | 3 N·m | 27 lb in
Front Muffler-to-Rear Muffler Nut | 40 N·m | 30 lb ft
Front Support Bracket Bolt | 20 N·m | 15 lb ft
Fuel Tank Shield Retaining Nuts | 3 N·m | 27 lb in
Heater Adapter Bolt | 20 N·m | 15 lb ft
Idler Retaining Bolt | 45 N·m | 33 lb ft
Ignition Coil Bolt | 7 N·m | 62 lb in
Intake Air Temperature (IAT) Sensor | 25 N·m | 18 lb ft
Intake Manifold Retaining Bolt/Nut | 12 N·m | 106 lb in
Intake Manifold Support Bracket Bolt | 25 N·m | 18 lb ft
Knock Sensor | 19 N·m | 14 lb ft
Lower Pad Bracket Bolt | 40 N·m | 30 lb in
Manifold Absolute Pressure (MAP) Sensor Bolt | 8 N·m | 71 lb in
Oil Filter | 14 N·m | 124 lb in
Oil Filter Adapter Retaining Bolt | 23 N·m | 17 lb ft
Oil Pan Drain Plug | 35 N·m | 26 lb ft
Oil Pan Flange-to-Transaxle Bolt | 31 N·m | 23 lb ft
Oil Pan Retaining Bolt | 10 N·m | 89 lb in
Oil Pump Bolt | 20 N·m | 15 lb ft
Oil Pump Chain Lever Bolt | 8 N·m | 71 lb in
Oil Pump Sprocket Cover Bolt | 6 N·m | 53 lb in
Oil Pump Sprocket Retaining Nut | 20 N·m | 15 lb ft
Oil Suction Pipe Bracket Bolt | 10 N·m | 89 lb in
Oil Suction Pipe-to-Oil Pump Retaining Bolt | 10 N·m | 89 lb in
Oxygen Sensor | 39 N·m | 29 lb ft
PCV Valve Bolt | 10 N·m | 89 lb in
Power Steering Pump Retaining Bolt | 25 N·m | 18 lb ft
Radiator Bracket Bolt | 14 N·m | 124 lb in
Rear Muffler Heat Shield Nut | 3 N·m | 27 lb in
Rear Support Bracket Bolt, Intake Side | 10 N·m | 89 lb in
Rear Support Bracket Bolt, Exhaust Side | 22 N·m | 16 lb ft
Rear Transaxle Mount Bracket Bolt | 65 N·m | 48 lb ft
Rocker Arm Shaft Plug | 40 N·m | 30 lb ft
Spark Plug | 25 N·m | 18 lb ft
Starter Motor Mount-to-Engine Block Bolt | 45 N·m | 33 lb ft
Starter Motor Mount-to-Transaxle Bolt | 50 N·m | 37 lb ft
Target Wheel Bolt | 9 N·m | 80 lb in
Thermostat Housing Bolt | 10 N·m | 89 lb in
Throttle Body Bolt | 13 N·m | 115 lb in
Timing Chain Cover Bolt | 8 N·m | 71 lb in
Timing Chain Cover Bolt, Center | 20 N·m | 15 lb ft
Timing Chain Lever Bolt | 20 N·m | 15 lb ft
Timing Chain Tensioner Bolt | 20 N·m | 15 lb ft
Top Chain Guide Bolt | 10 N·m | 89 lb in
Transaxle Mount Cage Through Bolt | 110 N·m | 81 lb ft
Transaxle Mount Cage-to-Longitudinal Member Bolt | 65 N·m | 48 lb ft
Transaxle Mount Cage-to-Transaxle Mount Bracket Bolt | 65 N·m | 48 lb ft
Transaxle Mount Cage-to-Transaxle Mount Bracket Nut | 65 N·m | 48 lb ft
Transaxle Torque Converter Bolt | 45 N·m | 33 lb ft
Upper Pad Bracket Bolt | 45 N·m | 33 lb ft
Upper Pad-to-Lower Pad Bracket Bolt | 35 N·m | 26 lb ft
Water Pump Bolt | 23 N·m | 17 lb ft
Water Pump Pulley Bolt | 10 N·m | 89 lb in
Wiring Harness Bracket Bolt | 10 N·m | 89 lb in