For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the manifold absolute pressure (MAP) sensor connector.
3. Remove the MAP sensor.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the MAP sensor and tighten to 8 N·m (71 lb in).
2. Connect the MAP sensor connector.
3. Connect the negative battery cable.