For 1990-2009 cars

Callout | Component Name
--- | ---
1 | 3-5 Reverse and 4-5-6 Clutch Fluid Seals (Qty: 4) Tip

• | Discard the fluid seals. They are not reusable.

• | Refer to 3-5-Reverse and 4-5-6 Clutch Fluid Seal Ring Replacement .

2 | Input Shaft Support Bolts M6 x 50 (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten Tighten to 12 N·m (106 lb in)
3 | Input Shaft Support Tip Inspect the support for wear, damage or porosity.