For 1990-2009 cars

### Removal Procedure

1. Remove the control valve body cover. Refer to Control Valve Body Cover Installation.
2. Disconnect the shift position switch electrical connector (1).
3. Disconnect the output speed sensor electrical connector (2).
4. Disconnect the input speed sensor electrical connector (3).
5. Remove the control valve body bolts (1) M5 x 40.5.
6. Remove the control valve body bolts (2) M6 x 97.
7. Remove the control solenoid valve body and transmission control module (TCM) assembly (3).

Important: Use care when removing or installing the filter plate. A broken or missing retaining tab may not adequately secure the filter plate to the control solenoid valve assembly, resulting in possible damage or contamination.

Important: Discard the filter plate. It is not reusable. Inspect the pressure switch seals for damage or contamination. Replace the control solenoid valve assembly as necessary.

8. Remove the control solenoid valve assembly filter plate (4).

### Installation Procedure

Important: Use care when removing or installing the filter plate. A broken or missing retaining tab may not adequately secure the filter plate to the control solenoid valve assembly, resulting in possible damage or contamination.

1. Install a NEW control solenoid valve assembly filter plate (1) to prevent fluid leaks past the fluid seals.
2. Install the control solenoid valve body and TCM assembly (2).

Notice: Refer to Fastener Notice in the Preface section.

Important: Install all bolts before tightening, then tighten in the specified sequence.

3. Install the control valve body bolts (3) M5 x 40.5.

Tighten
Tighten the bolts in sequence to 8 N·m (71 lb in).

4. Install the control valve body bolts (4) M6 x 97.

Tighten
Tighten the bolts in sequence to 12 N·m (106 lb in).

5. Connect the input speed sensor electrical connector (3).
6. Connect the output speed sensor electrical connector (2).
7. Connect the shift position switch electrical connector (1).
8. Install the control valve body cover. Refer to Control Valve Body Cover Installation.
9. Reprogram the TCM with the correct calibration.

Important: After an internal transmission repair or internal part replacement, the service fast learn adapt procedure should be performed.

10. Perform the service fast learn adapt procedure. Refer to Service Fast Learn Adapts.