For 1990-2009 cars

### Removal Procedure

1. Remove the upper B-pillar trim panel. Refer to Center Pillar Upper Trim Panel Replacement .
2. Remove the bolts and the seat belt height adjuster.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt height adjuster with the bolts.

Tighten
Tighten the front seat belt height adjuster bolts to 38 N·m (28 lb ft).

2. Install the upper B-pillar trim panel. Refer to Center Pillar Upper Trim Panel Replacement .