For 1990-2009 cars

### Removal Procedure

1. Remove the door seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement.
2. Remove the exterior front door body side molding. Refer to Front Side Door Molding Replacement.
3. Remove the screws that secure the glass to the window regulator.
4. Remove the glass from the door.

### Installation Procedure

1. Install the glass in the door and position the glass within the window regulator.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the glass screws and tighten to 7 N·m (62 lb in).
3. Install the exterior front door body side molding. Refer to Front Side Door Molding Replacement.
4. Install the door seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement.