For 1990-2009 cars

Connector 1: | Fuse Block - Underhood Label
Connector 2: | Fuse Block - Underhood Bottom View
Connector 3: | Fuse Block - Underhood X1
Connector 4: | Fuse Block - Underhood X2
Connector 5: | Fuse Block - Underhood X3
Connector 6: | Fuse Block - Underhood X4
Connector 7: | Fuse Block - I/P Top View
Connector 8: | Fuse Block - I/P Wire Entry

### Fuse Block - Underhood Label

#### Fuse Block - Underhood Label Usage

No. | Fuse | Rating | Description
--- | --- | --- | ---
EF1 | HVAC BLWR Fuse | 30A | Blower Relay
EF2 | BCM BATT Fuse | 60A | Body Control Module (BCM) (ISU)
EF3 | ABS Fuse | 60A | Electronic Brake Control Module (EBCM)
EF4 | IGN1 Fuse | 30A | Ignition Switch
EF5 | PWR WIDW Fuse | 20A | Power Window/Door Lock Switch - Driver
EF6 | COOL FAN HI Fuse | 20A | Cooling Fan High Relay
EF7 | COOL FAN LOW Fuse | 20A | Cooling Fan Low Relay
EF8 | ST/IG2 Fuse | 30A | Ignition Switch, STARTER Relay
EF9 | SPARE Fuse | 15A | SPARE
EF10 | SPARE Fuse | 10A | SPARE
EF11 | SPARE Fuse | 20A | SPARE
EF12 | SPARE Fuse | 25A | SPARE
EF13 | SPARE Fuse | 30A | SPARE
EF14 | ABS WARNING Fuse | 10A | Not Used
EF15 | S/ROOF Fuse | 20A | Sunroof Module
EF16 | ABS Fuse | 15A | ABS Oil Feeding Connector, Electronic Brake Control Module (EBCM)
EF17 | HVAC BLWR Fuse | 15A | Headlamp - Left, Headlamp - Right
EF18 | DRIVER'S PWR WIDW Fuse | 20A | Window Motor - Driver (ABZ)
EF19 | PWR MIRROR Fuse | 10A | Multifunction Switch
EF20 | ILLUM RT Fuse | 10A | Headlamp - Right, Tail Lamp - Right, Turn Signal/Park Lamp - RF
EF21 | LCM Fuse | 30A | Multifunction Control Module (MCM)
EF22 | IP Fuse | 25A | Fuse Block - I/P
EF23 | STOP LAMPS Fuse | 20A | Stop Lamp Switch
EF24 | ILLUM LT Fuse | 10A | Headlamp - Left, Tail Lamp - Left, Turn Signal/Park Lamp - LF
EF25 | PWR SEAT Fuse | 30A | Power Seat Switch, Power Seat Test Connector
EF26 | FUEL Fuse | 20A | Fuel Sender Assembly
EF27 | ECM Fuse | 15A | Engine Control Module (Gasoline), ENGINE MAIN Relay, Automatic Transmission (MH7/MH8)
EF28 | IGN COIL Fuse | 20A | Ignition Coil 1-6 (Gasoline)
EF29 | HORN Fuse | 15A | HORN Relay
EF30 | ENG2 Fuse | 15A | Fuel Injector 1-6 (Gasoline), Engine Control Module (Diesel), Evaporative Emissions (EVAP) Canister Purge Valve Solenoid (Gasoline), Vehicle Speed Sensor (VSS) (M/T)
EF31 | ENG3 Fuse | 20A | Not Used
EF32 | -- | -- | Empty
EF33 | ENG1 Fuse | 15A | A/C COMPRESSOR Relay, Exhaust Gas Recirculation (EGR) Solenoid Valve, Engine Control Module (ECM), Generator, VIM Solenoid Valve, Heated Oxygen Sensors, Camshaft Position (CMP), Mass Air Flow (MAF) Sensor, Evaporative Emissions (EVAP) Canister Vent Valve Solenoid
EF34 | FRT FOG Fuse | 15A | FOG LAMP Relay
EF35 | LOW BEAM LT Fuse | 10A | Headlamp - Left
EF36 | PWR AMP Fuse | 20A | Power Amplifier (U63)
EF37 | LOW BEAM RT Fuse | 10A | Headlamp - Right, Multifunction Switch (TR6)
EF38 | -- | -- | Empty
EF39 | A/C CMPRSR Fuse | 10A | A/C COMPRESSOR Relay
-- | ALTERNATOR Fuse | 120A | Generator, Fuse Block - Auxiliary Underhood (Diesel)
-- | A/C COMPRESSOR Relay | -- | A/C Compressor Clutch, Engine Control Module (ECM)
-- | COOLING FAN CONTROL Relay | -- | Cooling Fan - Main
-- | COOLING FAN HIGH Relay | -- | Cooling Fan - Main
-- | COOLING FAN LOW Relay | -- | Cooling Fan - Auxiliary
-- | ENGINE MAIN Relay | -- | EF30 Fuse, EF31 Fuse, EF33 Fuse, A/C COMPRESSOR Relay, COOLING FAM HIGH Relay, COOLING FAN CONTROL Relay, COOLING FAN LOW Relay
-- | FOG LAMP Relay | -- | Front Fog Lamp - Left, Front Fog Lamp - Right
-- | FUEL PUMP Relay | -- | EF26 Fuse, EF28 Fuse
-- | HEADLAMP HIGH Relay | -- | EF17 Fuse
-- | HEADLAMP LOW Relay | -- | EF35 Fuse, EF37 Fuse
-- | HORN Relay | -- | Horn High, Horn Low, Horn Switch
-- | ILLUMINATION Relay | -- | EF20 Fuse, EF24 Fuse
-- | POWER WINDOW Relay | -- | EF18 Fuse, EF5 Fuse, EF19 Fuse
-- | STARTER Relay | -- | Starter

### Fuse Block - Underhood Bottom View

### Fuse Block - Underhood X1

#### Connector Part Information

- OEM: 15319896
- Service: N/A
- Description: 68-Way F Metri-Pack 280 Series (BK)

#### Fuse Block - Underhood X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1-A3 | -- | -- | Not Used
A4 | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage
L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
A5-A9 | -- | -- | Not Used
A10 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage (TR6)
D-GN | 189 | Headlamp Leveling Motor Supply Voltage (TR6)
A11-A12 | -- | -- | Not Used
B1-B4 | -- | -- | Not Used
B5 | D-GN | 59 | A/C Compressor Clutch Supply Voltage
B6-B7 | -- | -- | Not Used
B8 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
B9 | RD/WH | 340 | Battery Positive Voltage
B10 | -- | -- | Not Used
B11 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
B12 | -- | -- | Not Used
C1 | L-BU | 409 | Cooling Fan Motor Supply Voltage (1)
C2-C3 | -- | -- | Not Used
C4 | YE | 196 | Windshield Wiper Motor Park Switch Signal
C5 | PU | 34 | Front Fog Lamp Supply Voltage
PU | 34 | Front Fog Lamp Supply Voltage
C6-C7 | -- | -- | Not Available
C8-C10 | -- | -- | Not Used
C11 | WH | 504 | Cooling Fan Motor Low Reference (Gasoline)
L-BU | 409 | Cooling Fan Motor Supply Voltage (1) (Diesel)
C12 | -- | -- | Not Used
D1 | L-BU | 409 | Cooling Fan Motor Supply Voltage (1) (Diesel)
D2 | PU | 709 | Left Park Lamp Supply Voltage
D3 | BN/WH | 309 | Right Park Lamp Supply Voltage
D4 | -- | -- | Not Used
D5 | BN/WH | 312 | Right Headlamp Low Beam Supply Voltage
BN/WH | 312 | Right Headlamp Low Beam Supply Voltage (TR6/TQE)
D6-D7 | -- | -- | Not Available
D8 | BN/WH | 312 | Right Headlamp Low Beam Supply Voltage (TR6)
D9 | BK | 250 | Ground (Gasoline)
YE | 5358 | Cooling Fan Motor Supply Voltage (3) (Diesel)
D10-D11 | -- | -- | Not Used
D12 | YE | 261 | Arm Alarm Signal
E1 | RD/WH | 340 | Battery Positive Voltage
E2-E4 | -- | -- | Not Used
E5 | YE | 712 | Left Headlamp Low Beam Supply Voltage
E6-E9 | -- | -- | Not Used
E10 | PK/BK | 109 | Hood Ajar Switch Signal
E11 | GY | 532 | Cooling Fan Motor Supply Voltage (2)
E12 | OG | 228 | Windshield Washer Pump Control
F1-F5 | -- | -- | Not Used
F6 | D-GN | 29 | Horn Control
D-GN | 29 | Horn Control
F7 | -- | -- | Not Used
F8 | L-GN/BK | 735 | Outside Ambient Air Temperature Sensor Signal (C68)
F9 | -- | -- | Not Used
F10 | YE | 61 | Outside Ambient Temperature Sensor Low Reference (C68)
F11 | GY | 532 | Cooling Fan Motor Supply Voltage (2) (Diesel)
F12 | YE | 712 | Left Headlamp Low Beam Supply Voltage (w/o TR6)
BN/WH | 312 | Right Headlamp Low Beam Supply Voltage (TQE)

### Fuse Block - Underhood X2

#### Connector Part Information

- OEM: 15319895
- Service: N/A
- Description: 68-Way F Metri-Pack 280 Flexlock Series (GY)

#### Fuse Block - Underhood X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | D-GN | 335 | Low Speed Cooling Fan Relay Control
A2 | PK | 1846 | Supply Voltage
PK | 1846 | Supply Voltage (LBM)
A3 | -- | -- | Not Used
A4 | PK | 1846 | Supply Voltage (LBK)
PK | 1846 | Supply Voltage (LBK)
A5 | PK | 1846 | Supply Voltage (LBK/LBM)
PK | 1846 | Supply Voltage (LBK/LBM)
A6 | PU/WH | 67 | A/C Compressor Clutch Coil Supply Voltage
A7 | -- | -- | Not Used
A8 | L-GN/BK | 735 | Outside Ambient Air Temperature Sensor Signal (C68)
A9 | -- | -- | Not Used
A10 | YE | 61 | Outside Ambient Temperature Sensor Low Reference (C68)
A11 | D-BU | 473 | High Speed Cooling Fan Relay Control
A12 | YE | 712 | Left Headlamp Low Beam Supply Voltage
B1 | RD/WH | 440 | Battery Positive Voltage
B2 | PK | 1846 | Supply Voltage
B3-B4 | -- | -- | Not Used
B5 | PK | 1846 | Supply Voltage
PK | 1846 | Supply Voltage (LBK/LBM)
PK/WH | 1846 | Supply Voltage (LLW)
B6-B9 | -- | -- | Not Used
B10 | PK | -- | Ignition 1 Voltage
B11 | -- | -- | Not Used
B12 | D-BU | 1885 | Service Vehicle Soon Indicator Control (LBK/LBM)
PU/WH | 1885 | Service Vehicle Soon Indicator Control (LLW)
C1 | -- | -- | Not Used
C2 | PK | 1846 | Supply Voltage (LBM)
PK/WH | 1846 | Supply Voltage (LLW)
C3 | BN | 5069 | Engine Main Relay Coil Control (LBK/LBM)
GY/BK | 5069 | Engine Main Relay Coil Control (LLW)
C4-C5 | -- | -- | Not Used
C6-C7 | -- | -- | Not Available
C8 | D-GN/WH | 762 | A/C Request Signal
C9 | -- | -- | Not Used
C10 | PK | -- | Ignition 1 Voltage
C11 | PK | 539 | Run/Crank Ignition 1 Voltage (LBK/LBM)
PK/BK | 539 | Run/Crank Ignition 1 Voltage (LLW)
C12 | -- | -- | Not Used
D1 | BN/WH | 6281 | Fuel Level Sensor Low Reference
D2 | PK | 1846 | Supply Voltage (LBK/LBM)
D3-D4 | -- | -- | Not Used
D5 | PK | 139 | Run/Crank Ignition 1 Voltage
D6-D7 | -- | -- | Not Available
D8 | -- | -- | Not Used
D9 | D-GN/WH | 465 | Fuel Pump Primary Relay Control
D10 | PK | 539 | Run/Crank Ignition 1 Voltage (LBK/LBM)
D11-D12 | -- | -- | Not Used
E1 | PU | 6 | Starter Solenoid Crank Voltage
E2 | YE | 30 | Fuel Level Sensor Signal (LBK/LBM)
E3 | PK | 139 | Run/Crank Ignition 1 Voltage (LBK/LBM)
PK/BK | 139 | Run/Crank Ignition 1 Voltage (LLW)
E4 | PK/BK | -- | Run/Crank Ignition 1 Voltage (LLW)
E5 | -- | -- | Not Used
E6 | PK | 139 | Run/Crank Ignition 1 Voltage (LBK/LBM)
PK/BK | 139 | Run/Crank Ignition 1 Voltage (LLW)
E7-E10 | -- | -- | Not Used
E11 | PK | 539 | Run/Crank Ignition 1 Voltage (LBK/LBM)
BK/WH | -- | Ground (LLW)
E12 | -- | -- | Not Used
F1 | OG/BK | 1786 | Transmission Park/Neutral Signal (1) (M98/MH7/MH8)
BK | 350 | Ground (MFB/MFN)
F2 | D-GN | 135 | Engine Coolant Temperature Gauge Signal
F3 | -- | -- | Not Used
F4 | L-GN | 24 | Backup Lamp Supply Voltage (MFB/MFN)
YE | 712 | Left Headlamp Low Beam Supply Voltage (LBK)
F5 | -- | -- | Not Used
F6 | PK/BK | -- | Run/Crank Ignition 1 Voltage (LLW)
F7-F9 | -- | -- | Not Used
F10 | PK | 739 | Run/Crank Ignition 1 Voltage
F11 | RD/WH | 440 | Battery Positive Voltage
F12 | WH/BK | 5043 | Serial Data

### Fuse Block - Underhood X3

#### Connector Part Information

- OEM: 15319894
- Service: N/A
- Description: 68-Way F Metri-Pack 280 Flexlock Series (NA)

#### Fuse Block - Underhood X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | YE | 5 | Crank Voltage
A2 | D-GN | 135 | Engine Coolant Temperature Gauge Signal
A3 | BN/WH | 99 | Windshield Washer Fluid Level Sensor Signal
A4 | L-GN | 24 | Backup Lamp Supply Voltage (MFB/MFN)
A5 | D-GN/WH | 1317 | Fog Lamp Relay Control
A6 | BN | 28 | Horn Relay Control
BN | 28 | Horn Relay Control
A7 | -- | -- | Not Used
A8 | OG | 340 | Battery Positive Voltage
A9 | -- | -- | Not Used
A10 | GY | 120 | Fuel Pump Supply Voltage
A11 | -- | -- | Not Used
A12 | OG/BK | 740 | Battery Positive Voltage
B1-B4 | -- | -- | Not Used
B5 | PU | 709 | Left Park Lamp Supply Voltage
B6 | PK | 539 | Run/Crank Ignition 1 Voltage
B7 | OG | 540 | Battery Positive Voltage
B8-B9 | -- | -- | Not Used
B10 | RD/BK | 242 | Battery Positive Voltage
B11 | RD/WH | 1340 | Battery Positive Voltage
B12 | -- | -- | Not Used
C1 | -- | -- | Not Used
C2 | OG | 55 | Fuel Gauge Signal
C3 | WH | 1080 | Park Lamp Relay Control
C4 | -- | -- | Not Used
C5 | BN/WH | 309 | Right Park Lamp Supply Voltage
C6-C7 | -- | -- | Not Available
C8 | D-GN/WH | 762 | A/C Request Signal
C9 | BN | 1739 | Run/Crank Ignition 1 Voltage
C10-C11 | -- | -- | Not Used
C12 | OG | 1580 | Fuel Pump Low Reference
D1 | -- | -- | Not Used
D2 | BN | 189 | Headlamp Leveling Motor Supply Voltage (TR6)
D3-D4 | -- | -- | Not Used
D5 | D-GN/BK | 1798 | Low Reference
D6-D7 | -- | -- | Not Available
D8 | L-GN | 312 | Right Headlamp Low Beam Supply Voltage (TR6)
D9 | PK/BK | 109 | Hood Ajar Switch Signal
D10 | PK | 539 | Run/Crank Ignition 1 Voltage
PK | 539 | Run/Crank Ignition 1 Voltage
D11 | YE | 261 | Arm Alarm Signal
D12 | -- | -- | Not Used
E1 | BN | 41 | Run Ignition 3 Voltage
E2 | D-BU/WH | 1885 | Service Vehicle Soon Indicator Control
E3-E4 | -- | -- | Not Used
E5 | PK | 1339 | Run/Crank Ignition 1 Voltage
PK | 1339 | Run/Crank Ignition 1 Voltage
E6 | PK/WH | 2339 | Run/Crank Ignition 1 Voltage
E7 | RD/WH | 840 | Battery Positive Voltage
E8-E9 | -- | -- | Not Used
E10 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
E11 | -- | -- | Not Used
E12 | D-GN/BK | 2905 | Data Communication
F1 | -- | -- | Not Used
F2 | PU | 1589 | Primary Fuel Level Sensor Signal
F3 | RD/WH | 140 | Headlamp High Beam Relay Control
F4 | RD/BK | 642 | Battery Positive Voltage
F5-F9 | -- | -- | Not Used
F10 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
F11 | PK/D-BU | 638 | Power Window Enable Relay Control
F12 | OG | 228 | Windshield Washer Pump Control
OG | 228 | Windshield Washer Pump Control (CE1)

### Fuse Block - Underhood X4

#### Connector Part Information

- OEM: 15447740
- Service: N/A
- Description: 8-Way F Metri-Pack 800 Series (BK)

#### Fuse Block - Underhood X4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | OG | 580 | Battery Positive Voltage
A2 | RD/BK | 742 | Battery Positive Voltage
B1 | -- | -- | Not Used
B2 | RD | 142 | Battery Positive Voltage
C1 | -- | -- | Not Used
C2 | RD | 42 | Battery Positive Voltage
D1 | -- | -- | Not Used
D2 | RD/WH | 1642 | Battery Positive Voltage

### Fuse Block - I/P Top View

#### Fuse Block - I/P Label Usage

No. | Fuse | Rating | Description
--- | --- | --- | ---
F1 | CLUSTER2 Fuse | 10A | Driver Information Center (DIC), Instrument Panel Cluster (IPC), Multifunction Control Module (MCM), Park/Neutral Position (PNP) Switch (A/T), Remote Control Door Lock Receiver (RCDLR), Transmission Control Module (TCM) (A/T)
F2 | WIPER Fuse | 25A | Rain Sensor (CE1), Windshield Wiper Motor, Windshield Wiper/Washer Switch
F3 | ECU Fuse | 15A | Park/Neutral Position (PNP) Switch (A/T), Transmission Control Module (TCM) (A/T)
F4 | HVAC Fuse | 10A | Body Control Module (BCM), Blower Relay, HVAC Control Module, Mode Actuator, Recirculation Actuator
F5 | CLOCK Fuse | 10A | Clock, Multifunction Control Module (MCM), Sunroof Module, Front Dome Lamp
F6 | RADIO Fuse | 10A | Navigation Module, Radio
F7 | HEATING MAT Fuse | 20A | Heated Seat Switch - Driver, Heated Seat Switch - Passenger
F8 | AUDIO Fuse | 20A | Radio
F9 | CLUSTER1 Fuse | 10A | Clock, Driver Information Center (DIC), HVAC Control Module, Instrument Panel Cluster (IPC), Key Reminder Switch, Multifunction Control Module (MCM), Remote Control Door Lock Receiver (RCDLR)
F10 | SDM Fuse | 10A | Inflatable Restraint Sensing and Diagnostic Module (SDM)
F11 | AIR BAG Fuse | 10A | Passenger Air Bag/Seat Belt Warning Lamp, Passenger Presence Detection (PPS) Sensor
F12 | SPARE Fuse | 10A | Not Used
F13 | LCM Fuse | 10A | Multifunction Control Module (MCM) and Traction Control Switch (NW9)
F14 | CIGAR Fuse | 20A | Auxiliary Power Outlet and Cigar Lighter
F15 | SUB WOOFER Fuse | 20A | Subwoofer Speaker
F16 | B/UP LP Fuse | 15A | Back Up Lamp Switch (M/T), Inside Rearview Mirror, Instrument Panel Cluster (IPC), Object Detection Module, Park/Neutral Position (PNP) Switch (A/T), Shift Lever Selector, Stop Lamp Switch
F17 | U/H J/B Fuse | 15A | Automatic Transmission (MH7/MH8), Engine Control Module (ECM), FOG LAMP Relay, FUEL PUMP Relay, Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
F18 | ISU Fuse | 25A | Body Control Module (BCM), Windshield Wiper/Washer Switch
F19 | OSRVM Fuse | 10A | HVAC Control Module, Outside Rearview Mirror - Driver, Outside Rearview Mirror - Passenger
F20 | A/D CONVERTER Fuse | 15A | Not Used
F21 | SSPS Fuse | 15A | Power Steering Control Module (Gasoline), Clutch Start Switch (Diesel)
F22 | ALDL Fuse | 15A | Data Link Connector (DLC), Rear Compartment Release Switch, Transmission Control Module (TCM) (M98)
F23 | ESC Fuse | 30A | Electronic Brake Control Module (F45)

### Fuse Block - I/P Wire Entry

#### Connector Part Information

- OEM: 936195-1
- Service: N/A
- Description: 76-Way F 090/250 Hybrid Series (BK)

#### Fuse Block - I/P Wire Entry

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | RD/BK | 242 | Battery Positive Voltage
4 | -- | -- | Not Used
5 | RD/WH | 1840 | Battery Positive Voltage
RD/WH | 1840 | Battery Positive Voltage (A/T)
6 | RD/WH | 1840 | Battery Positive Voltage
7-9 | -- | -- | Not Used
10 | PK | 639 | Run/Crank Ignition 1 Voltage
11 | PK | 639 | Run/Crank Ignition 1 Voltage
12 | PU/WH | 1293 | --
13 | PK | 539 | Run/Crank Ignition 1 Voltage
14 | PK | 839 | Run/Crank Ignition 1 Voltage (A/T)
PK | 839 | Run/Crank Ignition 1 Voltage (A/T)
15 | PK | 839 | Ignition Voltage
PK | 839 | Ignition Voltage (M/T)
16-18 | -- | -- | Not Used
19 | BN | 141 | Run Ignition 3 Voltage
20-23 | -- | -- | Not Used
24 | OG | 267 | Mirror Heater Element Voltage
25 | PK | 839 | Run/Crank Ignition 1 Voltage
26-28 | -- | -- | Not Used
29 | RD/WH | 1740 | Battery Positive Voltage
30 | -- | -- | Not Used
31 | YE | 43 | Accessory Voltage (RHD)
32-34 | -- | -- | Not Used
35 | OG | 300 | Run Ignition 3 Voltage
36 | PK | 3 | Run/Crank Ignition 1 Voltage
37 | PK | 1139 | Run/Crank Ignition 1 Voltage
38 | -- | -- | Not Used
39 | RD/WH | 1140 | Battery Positive Voltage
40 | -- | -- | Not Used
41 | BN | 4 | Accessory Voltage
42-45 | -- | -- | Not used
46 | PK/BK | 1339 | Run/Crank Ignition 1 Voltage (NW9)
47 | YE | 143 | Accessory Voltage
48 | PK/WH | 2339 | Run/Crank Ignition 1 Voltage
49 | PK | 339 | Run/Crank Ignition 1 Voltage
50 | PK | 339 | Run/Crank Ignition 1 Voltage
51-53 | -- | -- | Not Used
54 | YE | 43 | Accessory Voltage (LHD)
55 | -- | -- | Not Used
56 | BN | 41 | Run Ignition 3 Voltage
57 | BN | 41 | Run Ignition 3 Voltage
58 | -- | -- | Not Used
59 | PK/D-BU | 145 | Ignition 2 Voltage
60 | PK | 239 | Ignition Voltage
PK | 239 | Ignition Voltage
61 | PK | 239 | Run/Crank Ignition 1 Voltage
PK | 239 | Run/Crank Ignition 1 Voltage
62-63 | -- | -- | Not Used
64 | OG | 40 | Battery Positive Voltage
65 | BN | 241 | Ignition Voltage
66 | YE | 243 | Accessory Voltage
YE | 243 | Accessory Voltage
67-68 | -- | -- | Not Used
69 | BN | 41 | Run Ignition 3 Voltage
70-71 | -- | -- | Not Used
72 | PK | 439 | Run/Crank Ignition 1 Voltage
73 | PK | 939 | Run/Crank Ignition 1 Voltage
74 | PK | 939 | Run/Crank Ignition 1 Voltage
75-76 | -- | -- | Not Used