For 1990-2009 cars

### Removal Procedure

Important: Left-Hand Drive Shown, Right-Hand Drive Similar.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screws and the cruise control switch.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the cruise control switch with the screws.

Tighten
Tighten the cruise control switch screws to 3 N·m (27 lb in).

3. Connect the negative battery.