For 1990-2009 cars

Application | Description
--- | ---
Nozzle Type | Full jet spray nozzle #1/2 GG-25 or equivalent with a 60° included angle
Nozzle Height | Approximately 1 600 mm (63 in) from the floor
Volume of Flow | 14L (3.7 gal) per minute
Pressure | 155 kPa (22.5 psi) measured at the nozzle
Windshield and Windshield Pillar Test Stand Position | Approximately 30° down, 45° toward the rear, and aimed at the corner of the windshield
Center Pillar Test Stand Position | Approximately 30° down, 45° toward the rear, and aimed at the corner of the rear door
Back Window and Rear Deck Lid Test Stand Position | Approximately 30° down, 30° toward the front and aimed approximately 610 mm (24 in) from the corner of the back window