For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the stabilizer shaft-to-stabilizer link nut and the shaft-to-strut assembly nut.
3. Remove the rear stabilizer link.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Install the rear stabilizer link with the stabilizer shaft-to-stabilizer link nut and the shaft-to-strut assembly nut and tighten to 50 N·m (37 lb ft).