For 1990-2009 cars

1. Rotate the transmission assembly so that the I.D. tag is facing up.
2. Install 2 new case fluid passage seals (86) into the transmission case fluid ports.
3. Shift the transmission into Neutral (N).
4. While holding the control valve body assembly (39), connect the manual valve link (336) to the manual shift detent lever assembly (710).
5. Install the 6 control valve body assembly to transmission case bolts and hand tighten.

• | 2 - M6 x 1.0 x 16 mm (34)

• | 2 - M6 x 1.0 x 28 mm (35)

• | 2 - M6 x 1.0 x 55 mm (47)

Caution: Refer to Fastener Caution in the Preface section.

6. Tighten the control valve body assembly to transmission case bolts in sequence and tighten to 10 N·m (89 lb in).
7. Install a new control valve body fluid passage cover gasket (38).
8. Install the control valve body fluid passage cover (37).
9. Install the 2 - M6 x 1.0 x 50 mm control valve body bolts and tighten to 10 N·m (89 lb in).