For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the air filter housing.
3. Remove the input speed sensor electrical connector (3) from the input speed sensor.
4. Remove the input speed sensor bolt.
5. Remove the input speed sensor from the transaxle.
6. Remove the input speed sensor O-ring. Discard the O-ring.

### Installation Procedure

1. Apply the transaxle fluid to the new input sped sensor O-ring.
2. Install the new input speed sensor O-ring onto the input speed sensor.
3. Install the input speed sensor to the transaxle.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the input speed sensor bolt and tighten to 6 N·m (53 lb in).
5. Connect the electrical connector (3) to the input speed sensor.
6. Install the air filter housing.
7. Connect the negative battery cable.