For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the stabilizer shaft-to-stabilizer link nut and the shaft-to-strut assembly nut.
3. Remove the rear stabilizer link.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Install the rear stabilizer link with the stabilizer shaft-to-stabilizer link nut and the shaft-to-strut assembly nut.

Tighten
Tighten the rear stabilizer link with the stabilizer shaft-to-stabilizer link nut and the shaft-to-strut assembly nut to 50 N·m (37 lb ft).