For 1990-2009 cars

### Removal Procedure

1. Remove the front molding (1) bonded by the two sided tape.
2. Remove the front lower fascia extension screws.
3. Remove the side lower screws from the front lower fascia extension.
4. Remove the side screws and the retaining clips from the front lower fascia extension.
5. Remove the nuts from the front lower fascia extension.
6. Remove the front lower fascia extension from the vehicle.

### Installation Procedure

1. Install the front lower fascia extension.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front lower fascia extension nuts.

Tighten
Tighten the front lower fascia extension nuts to 2 N·m (18 lb in).

3. Install the side screws and the lower retaining clips.

Tighten
Tighten the side screws to 2 N·m (18 lb in).

4. Install the lower fascia extension lower screws.

Tighten
Tighten the lower screws to 2 N·m (18 lb in).

5. Install the lower fascia extension screws.

Tighten
Tighten the lower screws to 2 N·m (18 lb in).

6. Apply new two way tape and install the front lower fascia extension molding (1).