For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the engine cover. Refer to Engine Cover Replacement.
3. Disconnect the EGR vacuum solenoid valve inlet/outlet hoses.
4. Disconnect the EGR vacuum solenoid valve connector.
5. Remove the EGR vacuum solenoid valve.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the EGR vacuum solenoid valve using the retaining bolts and tighten to 7 N·m (62 lb in).
2. Connect the EGR vacuum solenoid valve connector.
3. Connect the EGR vacuum solenoid valve inlet/outlet hoses.
4. Install the engine cover. Refer to Engine Cover Replacement.
5. Connect the negative battery cable.