For 1990-2009 cars

### Removal Procedure

1. Remove the bolt and the upper front seat belt anchor.
2. Reposition the upper portion of the lower center pillar.
3. Pry off the upper center pillar trim panel.

### Installation Procedure

1. Install the upper center pillar trim panel.
2. Install the upper portion of the lower center pillar trim panel to its original position.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the upper front seat belt anchor with the bolt and tighten to 38 N·m (28 lb ft).