For 1990-2009 cars

#### Special Tools

• | J 34730-1A Fuel Pressure Gage

• | J 42982 Fuel Pressure Gage Adapter

• | CH-47831 Fuel Line Disconnect Tool

### Installation Procedure

1. Relieve the fuel pressure. Refer to Fuel Pressure Relief .
2. Remove the fasteners from the engine cover.
3. Remove the engine cover from the engine.
4. Disconnect the quick connect coupling of the fuel feed hose (3) from the fuel feed pipe of the fuel rail. Use a shop towel in order to catch any remaining fuel that may leak.
5. Install the J 42982 between the fuel feed pipe of the fuel rail and of the fuel feed hose.
6. Install the J 34730-1A to the J 42982 , and tighten securely.
7. Install fuel pump fuse.
8. Turn ON the ignition in order to pressurize the fuel system.
9. Turn OFF the ignition.
10. Check for any fuel leaks.

### Removal Procedure

1. Relieve the fuel pressure. Refer to the Fuel Pressure Relief .
2. Remove the J 34730-1A from the J 42982 .
3. Using the CH-47831 , disconnect the quick connect coupling of the J 42982 from the fuel feed pipe of the fuel rail. Use a shop towel in order to catch any remaining fuel that may leak.
4. Disconnect the quick connect coupling of the fuel feed hose (3) from the J 42982 , and remove the adapter. Use a shop towel in order to catch any remaining fuel that may leak.
5. Connect the quick-connect fitting of the fuel feed hose (3) to the fuel feed pipe of the fuel rail.
6. Install fuel pump fuse.
7. Turn ON the ignition in order to pressurize the fuel system.
8. Turn OFF the ignition.
9. Check for any fuel leaks.
10. Install the engine cover.
11. Secure the engine cover with the fasteners.

Tighten
Tighten the fasteners to 10 N·m (89 lb in).