For 1990-2009 cars

### Removal Procedure

1. Remove the rear door glass. Refer to Rear Side Door Window Replacement .
2. Remove the bolts and the screw from the rear door quarter window guide rail.
3. Remove the guide rail and the rear door quarter window.

### Installation Procedure

1. Install the guide rail and the rear door quarter window.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear door quarter window guide rail bolts and the screw.

Tighten

• | Tighten the guide rail bolts to 10 N·m (89 lb in).

• | Tighten the guide rail screw to 4 N·m (35 lb in).

3. Install the rear door glass. Refer to Rear Side Door Window Replacement .