For 1990-2009 cars

1. Perform a preliminary inspection before any attempt is made to change or correct the wheel alignment factors. Refer to Preliminary Alignment Inspection .
2. Loosen the front parallel link cam bolt to crossmember.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the front parallel link cam bolt.

Tighten
Tighten the bolt to 40 N·m (30 lb ft).

4. Adjust the rear toe specification. Refer to Wheel Alignment Specifications for preferred specifications.
5. Tighten the front parallel link cam bolt.

Tighten
Tighten the bolt to 80 N·m (59 lb ft).