For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the camshaft position (CMP) sensor connector.
3. Remove the CMP sensor.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the CMP sensor using the retaining bolt and tighten to 12 N·m (106 lb in).
2. Connect the CMP sensor connector.
3. Connect the negative battery cable.