For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the screws from the rear console compartment. Remove the compartment. Refer to Front Floor Console Replacement.
3. Remove the automatic console cap.
4. Remove the floor console cover.
5. Remove the console lamp and disconnect the electrical connector.
6. Remove the screws and the ashtray trim panel.
7. Disconnect the electrical connectors to the trim panel.
8. Remove the heated seat switch.

### Installation Procedure

1. Install the heated seat switch.
2. Connect the electrical connectors to the ashtray trim panel.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the trim panel and secure with the screws.

Tighten
Tighten the screws to 2.5 N·m (22 lb in).

4. Connect the console lamp connector and install the console lamp.
5. Install the floor console cover.
6. Install the automatic console cap.
7. Install the rear console compartment. Install the screws to the compartment. Refer to Front Floor Console Replacement.
8. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.