For 1990-2009 cars

### Removal Procedure

1. Remove the crossmember.
2. Remove the stabilizer link.
3. Remove the stabilizer bar bolts and nuts.
4. Remove the U-clamp and bushing.

### Installation Procedure

1. Install the U-clamp and bushing with stabilizer bar.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the stabilizer bar bolts and nuts and tighten to 50 N·m (37 lb ft).
3. Install the stabilizer link and crossmember.