For 1990-2009 cars

### Removal Procedure

1. Remove the driver seat. Refer to Front Seat Replacement - Bucket .
2. Remove the front seat cushion. Refer to Front Seat Cushion Replacement .
3. Disconnect the electrical connector.
4. Remove the bolts the screws, and the slide assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the slide assembly with the bolts and the screws.

#### Tighten

• | Tighten the slide assembly bolts to 25 N·m (18 lb ft).

• | Tighten the slide assembly screws to 10 N·m (89 lb in).

2. Connect the electrical connector.
3. Install the front seat cushion. Refer to Front Seat Cushion Replacement .
4. Install the driver seat. Refer to Front Seat Replacement - Bucket .