For 1990-2009 cars

## Clutch Does Not Disengage D33 Manual Transaxle

Checks | Actions
--- | ---
Check for the driver improperly operating the vehicle. | Correct the driver's operation of the vehicle as necessary.
Check for the insufficient oil or the leak at the oil pressure line. | Repair the leak or add the oil.
Check for a warped or worn clutch disc. | Replace the necessary clutch components. Refer to Clutch Assembly Replacement .
Check for worn splines on the input shaft. | Repair or replace the splines on the input shaft.
Check for a weak diaphragm spring. | Replace the necessary clutch components.

## Clutch Does Not Disengage D24 Manual Transaxle

Checks | Actions
--- | ---
DEFINITION: When the pedal is pressed to the floor, the shift lever does not move freely in and out of reverse gear.
Check for a damaged clutch disc. | Replace the damaged clutch disc.
Check for an improperly installed fork shaft. | Remove and properly reinstall the fork shaft. Very lightly lubricate the fork fingers at the release bearing with wheel bearing grease.
Check for the clutch disc hub binding on the input shaft spines. | Repair or replace the clutch disc hub.
Check for a warped or bent clutch disc. | Replace the warped or bent clutch disc.