For 1990-2009 cars

Checks | Causes
--- | ---
4-5-6 Clutch Assembly |

• | Inspect for leaking or damaged 4-5-6 Clutch Piston (520) and Piston Seals (518, 519, 521)

• | Inspect for plugged or restricted 4-5-6 Piston Dam air bleed

• | Inspect for leaking or damaged 4-5-6 Clutch Dam (523)

• | Inspect for plugged or restricted Dam oil feed hole in the 4-5-6 Piston (520)

• | Inspect for fatiqued 4-5-6 Clutch Piston Spring (522)

• | Inspect for leaking 4-5-6 Clutch Dam Seals (523)

• | Inspect for improper surface finish on 4-5-6 Clutch Plates (525-528)

• | Inspect for fatigued 4-5-6 Clutch Waved Plate (525)

• | Inspect for porous, improper surface finish, seal groove damage or plugged or restricted oil passages of the 3-5 Rev/4-5-6 Housing (516)