For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Support Fixture

### Removal Procedure

1. Remove the air filter housing.
2. Install the DW-110-060 .
3. Support the transaxle with a supporting jack.
4. Remove the left 3 transaxle mounting bracket bolts.
5. Remove the transaxle mounting bracket cage bolt and nut.
6. Remove the left transaxle mounting bracket.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the left transaxle mounting bracket and the 3 transaxle mounting bracket bolts and tighten to 40 N·m (30 lb ft).
2. Install the transaxle mounting bracket cage bolt and nu t and tighten to 65 N·m (48 lb ft).
3. Remove the DW-110-060 .
4. Install the air filter housing.