For 1990-2009 cars

Warning: Valve springs can be tightly compressed. Use care when removing retainers and plugs. Personal injury could result.

1. Remove the spacer plate and gasket assembly (324) from the rear control valve body assembly (326).
2. Remove the 7 rear valve body cover plate bolts (421).
3. Remove the rear valve body cover plate (420).
4. Remove the rear valve body cover plate gasket (419).
5. Remove the secondary regulator valve spring (437).
6. Remove the secondary regulator valve (436).
7. Remove the line pressure control (SLT) accumulator piston spring - inner (435).
8. Remove the line pressure control (SLT) accumulator piston spring - outer (434).
9. Remove the line pressure control (SLT) accumulator piston (433).
10. Remove the shift pressure control valve plunger sleeve (432).
11. Remove the shift pressure control valve plunger (431).
12. Remove the shift pressure control valve (430).
13. Remove the shift pressure control valve spring (429).
14. Remove the shift pressure control valve sleeve (428).
15. Remove the M2 shift valve spring (427).
16. Remove the M2 shift valve (426).
17. Remove the shift pressure relay valve spring (425).
18. Remove the shift pressure relay valve (424).
19. Remove the third gear band (B4) control valve (423).
20. Remove the third gear band (B4) control valve spring (422).
21. Remove the 2 rear valve body cover plate bolts (416).
22. Remove the rear valve body cover plate (417).
23. Remove the rear valve body cover plate gasket (418).
24. Remove the lock up relay control valve sleeve (412).
25. Remove the lock up relay control valve plunger (413).
26. Remove the lock up relay valve spring (414).
27. Remove the lock up relay valve (415).
28. Remove the 1-2 reverse clutch (B5) control valve (411).