For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door glass. Refer to Front Side Door Window Replacement.
3. Disconnect the electrical connector.
4. Remove the nuts and the window regulator.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the window regulator with the nuts and tighten to 10 N·m (89 lb in).
2. Connect the electrical connector.
3. Install the door glass. Refer to Front Side Door Window Replacement.
4. Connect the negative battery cable.