For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .
2. Pry off the vents by inserting a screwdriver.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Press the vents onto the housing.

Tighten
Tighten the instrument panel vent screws to 3 N·m (27 lb in).

2. Install the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .