For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement.
3. Remove the screws and the front door lock.
4. Disconnect the lock rods.
5. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Connect the lock rods.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the front door lock with the screws and tighten to 8 N·m (71 lb in).
4. Install the seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement.
5. Connect the negative battery cable.