For 1990-2009 cars

Checks | Actions
--- | ---
Check for worn or loose front wheel bearings. | Replace the front wheel bearings.
Check for a loose steering gear mounting. | Tighten the steering gear mounting bracket nuts and the bolts.
Check the joint from the column to the steering gear for loose connections or wear. |

• | Tighten the intermediate shaft pinch bolts.

• | Replace the intermediate shaft, as needed.

Check the steering gear preload adjustment. | Perform a rack bearing preload adjustment.