For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the cargo area rear trim panel. Refer the Cargo Area Rear Trim Panel Replacement .
3. Remove the SSPS control module bolts.
4. Slide the module up in order to remove the module.
5. Disconnect the electrical connector from the module.

### Installation Procedure

1. Connect the electrical connector to the SSPS control module.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the SSPS control module with bolts.

Tighten
Tighten the SSPS control module bolts to 9 N·m (80 lb in).

3. Install the cargo area rear trim panel. Refer to Cargo Area Rear Trim Panel Replacement .
4. Install the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .