For 1990-2009 cars

### Removal Procedure

1. Remove the engine shield. Refer to Engine Shield Replacement .
2. Remove the bolts and reposition the power steering return line.
3. Remove the forward engine mount-through bolt.
4. Remove the rear engine mount-through bolt.
5. Remove the bolts and the center member.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the center member with the bolts.

Tighten

• | Tighten the center member-to-crossmember bolt to 90 N·m (66 lb ft).

• | Tighten the center member-to-radiator bolt to 90 N·m (66 lb ft).

2. Install the rear engine mount-through bolt.

Tighten
Tighten the rear engine mount-through bolt to 80 N·m (59 lb ft).

3. Install the forward engine mount-through bolt.

Tighten
Tighten the forward engine mount-through bolt to 80 N·m (59 lb ft).

4. Install the power steering return line to its original position and install the bolts.
5. Install the engine shield. Refer to Engine Shield Replacement .

Tighten
Tighten the power steering return pipe fixing bolts to 7 N·m (62 lb in).